**Main Stage**

Stage lighting:

# Stage level – circuits in wells:

8 circuits - fixed floor

8 circuits- large revolving floor

# Gap above the auditorium - 22 circuits

10x ADB PC 2 kW

12x WARP 800W

# Ramp above the auditorium – 3 circuits

3x WARP 800W

# Ramp behind the auditorium – 4 circuits

7x WARP 800W

# Left hand side slots

# - 8 circuits

8x WARP 800W

# Right hand side slots - 8 circuits

8x WARP 800W

# Portal bridge - 14 circuits

8x ADB PC 1,2 kW

4x ADB PC 650W

2x warp 800W

# I light bridge - 13 circuits

4x ADB PC 2 kW

5x SPOTLIGHT PC 1200W

2x WARP 800W

# light bridge - 11 circuits

6x ADB PC 2 kW

4x SPOTLIGHT PC 1200W

1x WARP 800W

# light bridge - 6 circuits

3x ADB PC 2 kW

3x WARP 800W

# Gallery Third floor - left hand side – 5 circuits

5x WARP 800W

# Gallery Third floor - right hand side – 5 circuits

5x WARP 800W

# Backstage - 15 circuits

**Stage Level - Left hand side - 5 circuits**

5x ADB PC 650W

# Stage Level - Right hand side- 5 circuits

5x ADB PC 650W

# Portal tower - left hand side- 3 circuits

3x I PC 650W

# Portal tower – right hand side - 3 circuits

3x I PC 650W

# Auditorium lighting - 12 circuits

# Moving Head Light

2x Robe Wash 700E 2x Color Spot1200AT 4x ARIA 700 Profil

# Other:

Flood light- LED Spectra Cyc 100 RGBA – 6 pcs.

Strobe light FL1500 DMX -1psc.

# Setpoint:

Console ETC CONGO 1000 with wireless control

# Plug sockets - EBERLE type, possibly adapters

# Thyristor power controller- RP-2500 -/2.5 kW/

**Multimedia Projector:**

PANASONIC PT-5700E

# Effect Smoke Machine:

MARTIN MAGNUM PRO 2000 - 1 szt.

**Electroacoustics:**

Mixing console

Soundrcaft Vi 1, Stagebox 16/32

Sound system

FOH – 2 x JBL (2xVP7212/95DP)

SUB – 2 x JBL (2x VRX 918 SP) INFILL – 2x JBL AC28/26 SIDEFILL – 2x JBL AC15

Auditorium

JBL AC25

Monitors on stage

2x JBL PRX 612M

 5x JBL PRX 512M

2x Pol-Audio M110CX

Wireless sets

22 x SHURE ULX-D (bodypack)

2x SHURE Beta 58A

Players

TASCAM SS-CDR1

TASCAM SS-R1